***tcyiqj lgdkjh nqX/k la?k e;kZfnr***

**djkSank ukyk] bekfy;k] tcyiqj&482004 ¼e-iz-½**

**bZ&fufonk izi=**

**dqlhZ Vscy] vyekjh] ckWDl dz; gsrq bZ&fufonk lwpuk**

**fufonk [kqyus dk fnukad & 30-07-2020**

|  |
| --- |
| **tcyiqj lgdkjh nqX/k la?k e;kZfnr**  **djkSank ukyk bekfy;k tcyiqj&483220 ¼e-iz-½**  **Qksu ua- % Toll Free No. 9406900500**  **E-Mail : -** [**jdssanchi@gmail.com**](mailto:jdssanchi@gmail.com) |

**fufonk izi= dk ewY; :- 1000-00 ¼:i;s ,d gtkj ek=½**

 tcyiqj lgdkjh nqX/k la?k e;kZfnr

**Ms;jh la;a=%&** djkSank ukyk befy;k] tcyiqj ¼e-iz-½& 482004

**nwjHkk"k%&** 9406900500 **bZ esy%&** jdssanchi@gmail.com

**GST :** 23 AAAAJ0485D1Z6 (**An ISO**9001:2015 & 22000:2005 izekf.kr laLFkk½ **Pan :** AAAAJ0485D

**Øekad & 2026 @ts,lMh,l@ifj;kstuk@tcyiqj@2020 fnukad% 03-07-2020**

**&% bZ&fufonk lwpuk %&**

**tcyiqj lgdkjh nqX/k la?k e;kZfnr }kjk dqlhZ] Vscy] vyekjh] ckWDl dz; gsrq bZ&fufonk,W vkaef=r dh tkrh gS+ fufonk izi= fu/kkZfjr ewY; vkWuykbu tek dj csclkbV www.mptender.gov.in ls fnukad 08-07-2020 ls dz; fd;k tk ldrk gSA fufonk lEcaf/kr foLr`r fooj.k ,eih LVsV dks&vkijsfVo Ms;jh QsMjs’ku dh vf/kd`r csclkbV www.mpcdf.gov.in ij ns[kk ,oa i<k tk ldrk gSA fufonk izi= fodz; dh vafre fnukad 29-07-2020 le; nksigj 12%00 cts rd gSA**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **dzekad** | **fooj.k** | **ek=k** | **vekur jkf’k** | **fufonk izi= dz; jkf’k** |
|  | **dqlhZ] vkfQl Vscy] vyekjh] fVu ckWDl** | **vko';drk vuqlkj** | **:- 20]000-00** | **:- 1000-00** |

**eq[; dk;Zikyu vf/kdkjh**

 tcyiqj lgdkjh nqX/k la?k e;kZfnr

**Ms;jh la;a=%&** djkSank ukyk befy;k] tcyiqj ¼e-iz-½& 482004

**nwjHkk"k%&** 9406900500 **bZ esy%&** jdssanchi@gmail.com

**GST :** 23 AAAAJ0485D1Z6 (**An ISO**9001:2015 & 22000:2005 izekf.kr laLFkk½ **Pan :** AAAAJ0485D

**Øekad & 2026 @ts,lMh,l@ifj;kstuk@tcyiqj@2020 fnukad% 03-07-2020**

|  |  |  |
| --- | --- | --- |
| **fufonk izi=**  **fufonk dk;Z & dqlhZ] Vscy] vyekjh] ckWDl iznk;A** | | |
|  | **bZ&fufonk izi= dk ewY;** | :- 1000-00@&  ¼v{kjh& :i;s ik¡p lkS ek=½ |
| 1 | fufonk izi= fodz; izkjaHk djusa dh fnukad ,oa le;A | fnukad 08-07-2020 nksigj % 12%00 cts ls |
| 2 | fufonk izi= fodz; djusa dh vafre fnukad ,oa le; | fnukad 29-07-2020 nksigj % 12%00 cts rd |
| 3 | fufonk izi= Hkjusa dh vafre fnukad ,oa le; | fnukad 29-07-2020 nksigj % 12%00 cts rd |
| 4 | rduhdh fcM [kksyus dh vafre frfFk ,oa le; | fnukad 30-07-2020 nksigj % 3%00 cts |
| 5 | nj izi= [kksyus dh frfFk ,oa le; | Rkduhdh fcM esa ik= fufonkdkjksa dks izFkd ls lwfpr fd;k tkosxkA |
| 7 | i= O;ogkj ,oa fufonk [kqyus dk LFkku | eq[; dk;Zikyu vf/kdkjh tcyiqj lgdkjh nqX/k la?k e;kZfnr] djkSank ukyk befy;k] tcyiqj ¼e-iz-½& 482004  Contact No. 9399852009 |
| 8 | vekur jkf’k | :- 20]000-00 ¼:i;s chl gtkj ek=½ |
| 9 | layXu izi= | ifjf'k"V&d lkekU; fu;e@’krZ  ifjf'k"V&[k fufonkdkj ds fooj.k  ifjf'k"V&x nj izi= |
|  |  |  |

**eq[; dk;Zikyu vf/kdkjh**

**tcyiqj lgdkjh nqX/k la?k e;kZfnr] tcyiqj**

 tcyiqj lgdkjh nqX/k la?k e;kZfnr

**Ms;jh la;a=%&** djkSank ukyk befy;k] tcyiqj ¼e-iz-½& 482004

**nwjHkk"k%&** 9406900500 **bZ esy%&** jdssanchi@gmail.com

**GST :** 23 AAAAJ0485D1Z6 (**An ISO**9001:2015 & 22000:2005 izekf.kr laLFkk½ **Pan :** AAAAJ0485D

**Øekad & 2026 @ts,lMh,l@ifj;kstuk@tcyiqj@2020 fnukad% 03-07-2020**

**ifjf'k"V & d**

**fu;e ,oa 'krZs**

1. **vkWuykbu bZ&fufonk izi= izkIr djusa gsrq jkf’k :-1000-00 vkWuykbu tek dj fu/kkZfjr le; ls csclkbV www.mptender.gov.in ls izkIr dh tk ldrh gS] ,oa iw.kZ Hkjk gqvk rduhdh ,oa nj izi= fu/kkZfjr le; lhek esa vkWuykbu tek fd;k tkuk gSA**
2. **leLr nLrkost vkWuykbu tek djusa gksxsaA ftlesa th,lVh uEcj] isu uEcj] jftLVsª’ku lfVZfQdsV] dh Nk;kizfr vkWuykbu viyksM djuk vko’;d gSA**
3. **¼v½ ,d O;fDr@laLFkk }kjk dsoy ,d gh nj izi= izLRkqr dh tk;sA lQy nj izLrqr djusa okys fufonkdkj dks dk;Z vkns’k izlkfjr fd;s tkus ds mijkar mDr dk;Z vU; fdlh lsok iznk;drkZ dks gLrkarfjr ¼**Sublet**½ ugh fd;k tk ldrk gSA**

**¼c½ ,d O;fDr@laLFkk }kjk ,d ls vf/kd vyx&vyx ukeksa ls izLrqr dh xbZ fufonk nj dks Lohdkj ugh fd;k tk;sxkA**

1. **nqX/k la?k esa izkIr fdlh Hkh fufonk izi= dks leLr vFkok vkaf’kd :i ls Lohdkj vFkok vLohdkj djusa dk vf/kdkj eq[; dk;Zikyu vf/kdkjh egksn; tcyiqj lgdkjh nqX/k la?k e;kZfnr] tcyiqj ds ikl lqjf{kr jgsxkA ,d vFkok leLr fufonk izi= dks fujLr fd;s tkus ij dkj.k crk;s tkusa gsrq eq[; dk;Zikyu vf/kdkjh vFkok tcyiqj lgdkjh nqX/k la?k ck/; ugh jgsaxs- nqX/k la?k ds }kjk bl laca/k esa fdlh izdkj dk i=kpkj ugh fd;k tk;sxkA**
2. **nj izLrqrdrkZ dks pkgh xbZ leLr tkudkjh vfuok;Z :i ls Hkjuk gksxkA viw.kZ vFkok dkVNkWV fd;s x;s nj izi= dks ekU; ugh fd;k tk;sxkA**
3. **izkIr nj dh vof/k ,d o"kZ rd ekU; jgsxhA mDr nj vof/k dks dk;Z larq"V jgus ij vkilh lgefr ls lkeku nj ,oa fu;e 'krZ vuqlkj ,d&,d o"kZ dj vkxkeh nks o"kZ gsrq c<k;k tk ldsxkA dk;Z vof/k ds nkSjku nj esa o`f} ugh dh tk;sxhA**
4. **nj izLrqrdrkZ dks For- Jabalpur dairy plant Jabalpur leLr dj lfgr nj izLrqr djuk gSA**
5. **fufonk ,oa nj izi= [kqyus ds 15 fnol ds vUnj nj vueksnu dh lwpuk izsf"kr dh tk;sxhA**
6. **nj izi= ds fu;e ,oa 'krksZ dk ikyu ds laca/k esa mRiUu fdlh Hkh fookn ds fujkdj.k ds laca/k esa v/;{k ¼ps;j esu½ tcyiqj lgdkjh nqX/k la?k e;kZfnr] tcyiqj dk fu.kZ; vafre ,oa nksuksa i{kksa dks ca/kudkjh gksxkA**
7. **fdlh Hkh fookn gsrq U;k;ky; {ks= tcyiqj jgsxkA**
8. **fufonk izLrqrdrkZ fufonk izi= ds izR;sd i`"Bksa ij gLrk{kj ,oa eqgj yxk;sA**
9. **iznk;drkZ dks fuekZrk gksus dk izek.k&i= fufonk ds lkFk izLrqr djuk vfuok;Z gS] rFkk ftyk m?kksx O;kikj dsUnz esa jfTkLVªMZ gkssA**
10. **QuhZpj iznk; ds mijkar QuhZpj dh xq.koRrk lgh ik;s tkus ds ckn gh Hkqxrku fd;k tkosxkA**

**eq[; dk;Zikyu vf/kdkjh**

**tcyiqj lgdkjh nqX/k la?k e;kZfnr] tcyiqj**

 tcyiqj lgdkjh nqX/k la?k e;kZfnr

**Ms;jh la;a=%&** djkSank ukyk befy;k] tcyiqj ¼e-iz-½& 482004

**nwjHkk"k%&** 9406900500 **bZ esy%&** jdssanchi@gmail.com

**GST :** 23 AAAAJ0485D1Z6 (**An ISO**9001:2015 & 22000:2005 izekf.kr laLFkk½ **Pan :** AAAAJ0485D

**Øekad & 2026 @ts,lMh,l@ifj;kstuk@tcyiqj@2020 fnukad% 03-07-2020**

**ifjf'k"V & [k**

**eq[; dk;Zikyu vf/kdkjh]**

**tcyiqj lgdkjh nqX/k la?k e;kZfnr]**

**tcyiqj ¼e-iz-½**

**egksn;]**

|  |  |  |
| --- | --- | --- |
| **1** | **nj izLrqrdrkZ dk uke@irk@nwjHkk"k dzekad@bZ&esy vkbZ-Mh-** |  |
| **2** | **D;k fufonk Loa; ds uke ;k lk>snkjh@daiuh ds uke Hkjk tk jgk gSA** |  |
| **3** | **lk>snkjh@daiuh dk gS rks] lk>snkjksa ds uke] irk] nwjHkk"k dzekad ,oa bZ&esy vkbZ-Mh- ,oa isu** |  |
| **4** | **fufonkdkj ds Loa;@lk>snkjh@daiuh dk isu uacj@lfoZl VSDl ,oa th,lVh uacj ¼izfrfyfi layXu djsa½ ;fn QeZ ikVZujf’ki esa gks] rks lHkh ikVZujksa dk isu uacj izLrqr djsaA** |  |

**¼izR;sd fufonkdkj mijksDr ok¡fNr tkudkfj;kas dh izek.k i= dh izfrfyfi vko’;d :i ls fufonk izi= ds lkFk layXu djsa½**

**eSa ------------------------------------------------------------------fuoklh---------------------------------------------------------------------------------ds }kjk lR;kfir djrk g¡w fd] mijksDr leLr tkudkjh iw.kZ :i ls lR; ,oa lgh gS rFkk esjh laLFkk vFkok QeZ dks lkeku dk;Z gsrq Cysd fyLVsM ugh fd;k x;k gSA**

**fnukad &**

**fufonkdkj ds gLrk{kj ,oa eqgj**

**JABALPUR SAHAKARI DUGDHA SANGH MARYDIT,**

**KARONDA NALA, IMLIYA JABALPUR- 482004 (M.P.)**

**ITEMS AND SPECIFICATIONS**

1. **PLAIN ALMIRAH**

**OVERALL SIZE (H)1270X(W)760X(L) 430 MM**

Material details

1. The overall design and appearance of cabinets shall be as per their respective figures.

2- The CR sheet used shall be of prime quality and thickness for 1.0mm

1. Each shelf shall be formed such that edges are bend two time at right angle. First bend 30 mm and sccond bend 8mm.
2. Door stiffener from inside to its full height in top hat section size 100 m width.
3. Lever rod shall be 12m round
4. 2 nos of hinges of size 75 mm lengthx1.6mm thk.
5. Brackets shall be made of 1.6mm of m.s sheet riveted or botted on each side of hinges.
6. Machine made lever plate (patla) with brass bush of good quality or machine made six lever type patla .patla shall be covered by box cover fitted with round head scnews.
7. For locking brss body Godrej type cabinet lock or cabinet lock. 6 lever die cast zinc alloy body of size (H) 65x (w) 50 mm fitted on four screws or GRACE lock falt keys in duplicate with key rings shall be provided.
8. Metalic key cover electroplated nickel/chrome on front side of the door shall be provided. 11- For door die cast chrome plated handle fitted with washer and double lock nut.
9. Leg height shall be 125xmmx75mm.
10. Alos nefer General requirements. For manufacturing & accessories/hardware tec.
11. **OFFCE TABLE**

**OVERALL SIZE (L) 1060X(W)600X (H) 690 MM**

Material details

1. Table top :- 18mm tick pl mdf board isi mark.
2. Lipping :- Teak wood half round 16 mm wide& 8mm thick minimum.
3. Drawer and :- Cr sheet 0.80 mm thick in maximum two pieces in

Cupboard box size 450(D)x350(w)x255(H) mm

1. Drawer size :- 400(L)x85(D)mm minimum.
2. Frame & :- ERW square pipe 25x25x1.25mm in size 965(L)x450(w) x672(H)mm Structure
3. Foot rest :- ERW square pipe 25x25x1.25mm in full length.
4. Also refer General Requinements for manufacturing & accessories/hardware tec.
5. **CABINETS PLAIN ALMIRAH**

**OVERALL SIZE (H)1980X(W)915X(L)480 MM**

Material details

1. The overall design and appearance of cabinets shall be as per their respective figures.

02- The CR sheet used shall be of prime quality and thickness for 1.0mm

1. Each shelf shall be formed such that edges are bend two time at right angle. First bend 30 mm and sccond bend 8mm.
2. Door stiffener from inside to its full height in top hat section size 100 m width.

05- Lever rod shall be 12m round

1. 2 nos of hinges of size 75 mm lengthx1.6mm thk.
2. Brackets shall be made of 1.6mm of m.s sheet riveted or botted on each side of hinges.
3. Machine made lever plate (patla) with brass bush of good quality or machine made six lever type patla .patla shall be covered by box cover fitted with round head scnews.
4. For locking brss body Godrej type cabinet lock or cabinet lock. 6 lever die cast zinc alloy body of size (H) 65x (w) 50 mm fitted on four screws or GRACE lock falt keys in duplicate with key rings shall be provided.
5. Metalic key cover electroplated nickel/chrome on front side of the door shall be provided.
6. For door die cast chrome plated handle fitted with washer and double lock nut.
7. Leg height shall be 125xmmx75mm.
8. Alos nefer General requirements. For manfufactruring & accessories/hardware tec.
9. **OFFCE TABLE**

**OVERALL SIZE (L) 1060X(W)600X (H) 690 MM**

Material details

1. Table top :- 18mm tick pl mdf board isi mark.
2. Lipping :- Teak wood half round 16 mm wide& 8mm thick minimum.
3. Drawer and :- Cr sheet 0.80 mm thick in maximum two pieces in

Cupboard box size 450(D)x350(w)x255(H) mm

11- Drawer size :- 400(L)x85(D)mm minimum.

1. Frame & :- ERW square pipe 25x25x1.25mm in size 965(L)x450(w) x672(H)mm Structure
2. Foot rest :- ERW square pipe 25x25x1.25mm in full length.
3. Also refer General Requinements for manufacturing & accessories/hardware tec.
4. **TIN BOX**

**OVERALL SIZE (L)685X(W)381X(H)305MM**

1) Body G. Psheet 0.55 mm thk. 2) 16 No Staple 3) Side Handle 100 mm

4) Top hat for resting the cover 5) Bottom out side support

Material Details:-

1. The Design & appearance of this Tin box shall be as shown in the fig.
2. Two stapies on front side size no 16
3. Two side handle 100 mm in length on each side.
4. Hinges. Two nos. tail type size 65 mmx 1 m thick
5. Stopper arrangement for cover 2 nos
6. One support from inside of the lid/ cover 100 mm wide lengh wise in top hat section.
7. Vertical support in lower portion of the box from inside two nos in each side size 75mm width. 8- Letter compartment size 150(L)x100(H)10mm gap on inner side of lid/cover.
8. Reveting and Gl wire used as per standard practice in cover out dide & body indie by sheet bending.
9. Bottom stifferners from out side two nos width wise of 75 mm width in the form of top hat section provided as per standard practice.
10. The cover/lid of the box shall have height/depth of 75mm&wire bening outside by sheet bending.
11. Complete box shall be made from 0.55mmthick GP sheet (24G) (Minimum)
12. Top hat section for lower body of size 12x18 mm shall be made of single piece same sheet in the box below mm form lower body top for resting the cover.
13. Bottom corss support depth wise riveted 4 nos without top hat section simply made by over grooving& erabosing.
14. Also refer General requirements for manufacturing & accessories/ hardware etc.
15. **OFFICE CHAIR (CONTINIOUS ARMS)**

**OVERALL SIZE (H)900/455X(W)500X(D)560MM**

Material details

1 – Frame:- ERW round pile 25 mmdiax2 0mm thick in one piece.

1. Seat & back:- teak wood section 45x22mm finsh section size duly only in teak polish the best quality high strength nylon/plastic cane wire shall be used the 6 nos of cane wire shall be passed in each hole of back and seat in seat front section to be doubled and rounded to as shown in the fig.
2. fitting:- Seat shall be fitted over flat size 35x4mm thick in depth wise of frame on both side with minimum 3 nos screws on each side. Back rest shall be fitted by round heas stet screw 3 nos with suitable washer on each side.
3. Wooden handle:- Size 25x25x400mm made of teak wood with front curve having under side roved profile matching with pipe to be fitted with 3nos scnew on each side form underside handles shall be duty teak polished.
4. Also refer General requirements for manufacturing & accessories/ hardware etc

**eq[; dk;Zikyu vf/kdkjh**

 tcyiqj lgdkjh nqX/k la?k e;kZfnr

**Ms;jh la;a=%&** djkSank ukyk befy;k] tcyiqj ¼e-iz-½& 482004

**nwjHkk"k%&** 9406900500 **bZ esy%&** jdssanchi@gmail.com

**GST :** 23 AAAAJ0485D1Z6 (**An ISO**9001:2015 & 22000:2005 izekf.kr laLFkk½ **Pan :** AAAAJ0485D

**Øekad & 2026 @ts,lMh,l@ifj;kstuk@tcyiqj@2020 fnukad% 03-07-2020**

**ifjf'k"V & x**

**nj izi= %&**

**dqlhZ] Vscy] vyekjh] ckWDl**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **dzekad** | **LFkku** | **nj vadks esa** | **nj 'kCnksa esa** | **th-,l-Vh- nj** |
| **01** | Plain Almirah | **vkWuykbu viyksM djsaA** | **vkWuykbu viyksM djsaA** | **vkWuykbu viyksM djsaA** |
| **02** | Cabinets Plain Almirah | **vkWuykbu viyksM djsaA** | **vkWuykbu viyksM djsaA** | **vkWuykbu viyksM djsaA** |
| **03** | Office Table | **vkWuykbu viyksM djsaA** | **vkWuykbu viyksM djsaA** | **vkWuykbu viyksM djsaA** |
| **04** | Tin Box | **vkWuykbu viyksM djsaA** | **vkWuykbu viyksM djsaA** | **vkWuykbu viyksM djsaA** |
| **05** | Office Cahir  (Continious arms) | **vkWuykbu viyksM djsaA** | **vkWuykbu viyksM djsaA** | **vkWuykbu viyksM djsaA** |
|  | **nqX/k la;a= tcyiqj djkSank ukyk bekfy;k tcyiqj rd**  (For Jabalpur dairy Plant) |  |  |  |

**gekjs }kjk fufonk ds fu;e ,oa 'krsZ iwjh rjg ls i<+ yh xbZ gS] ,oa rnuqlkj njsa izLrqr dh xbZ gSA gekjs }kjk dk;Z vof/k ds nkSjku mijksDr njksa esa dksbZ ifjorZu ugha fd;k tk;sxkA**

**;g izi= Ldsu dj viyksM djsaA**

**gLrk{kj ,oa eqgj**